Triode for Alternating Current.

Property: (default value)

- Gate Resistance: (500 Ω)
   Gate to to MT1 Resistance.

- Holding Current: (10 mA)
   Minimum current to start conducing.

- Holding Current: (8.2 mA)
   Minimum current to keep conducing.


