Diode for Alternating Current.

Property: (default value)

- On Resistance: (500 Ω)
   Resistance when conducing.

- Off Resistance: (100 MΩ)
   Resistance when not conducing.

- Breakdwn Voltage (30 V)
    Voltage to start conducing.

- Holding Current: (10 mA)
   Minimum current to keep conducing.


